HiNC.20210604

1. create steps csv file by HiNC.
2. calculate temperature and other custom information by excel. 
3. Show those information in HiNC.




formula
=ABS(AC3)*(D3-D2)*para!B$8-(AO2-para!B$1)*para!B$5*0.001*para!B$2*(D3-D2)
=AN3/(para!B$6*(0.001*para!B$7))+AO2
=IF(ABS(AM2)>800,1,0)

para
normal temperature (K)	300	
heat transfer coefficient (W/mK)	58	(WC, 28~88)
cutter D (mm)	12	
cutter H (mm)	40	
cutter intersected area/height (mm)	2.827433388	
heat capacity (J/kgK)	240	(WC, 184~292)
local cutter weight (g)	0.07	(full cutter weight is 7)
heat conduct ratio from cutter to total	0.05	
